General Notes:
This project consists of furnishing and installing conduit, junction boxes, receptacles, data connectors, and cabling for connection to devices and to riser panels for the following buildings:
West Hospital
Cancer Clinic
Ambulatory Care
Nursing School
Conduit - 3/4" rigid metallic conduit from device receptacle to first junction box.
2" rigid metallic conduit from first junction box for the remainder of all conduit required.  
In general, run 2" conduit from first junction box to Riser panel on each floor with 2" conduit shunts between riser panels and MAU.
Junction boxes - All junction boxes to be 18"x18"x6" galvanized metal. Provide covers of same material. Junction boxes to meet all electrical code requirements. See plans for locations.